Meta Data

08/31/2007
48o 27.879  122o58.377

Scott, Ash, Sam, and Tim took dighy out bhind GV and measured receive levels at various distances with main generator on.  Props were not engaged.  We used Blue Box (calibrated InterOcean Systems hydrophone) and Marantz to record data files.  Tim processed data, saved under "processing" directory and "GV source level model" on data archive hard drive.  Raw data is in 070831 directory.